PS/PX/PC Series Powerstation Etherent Driver Options

12/06/2002  CTC Parker Automation

=====================================================================================

Two different Ethernet drivers are used with PowerStations.  The appropriate driver 
needs to be selected based on the processor type of the unit.

To use the drivers, browse to the appropriate folder and file listed.

266MHz Processor
 PS/PC/PX PowerStations with the following model number schemes have 266MHz
 processors:

     Pxxx-xx2-xxx-xxx  (Custom Configurations)
     Pxxx-xxxx-4           (Standard Configurations)

     For all Windows operating systems with 266Mhz Processor, please use the 
     following setup file:

		\\DRIVERS\PRO 100 ETHERNET\OEMSETUP.INF 


300MHz - 1.0GHz Processors
 PS/PC/PX PowerStations with the following model number schemes have 300MHz - 1.0GHz
 processors:

      Pxxx-xx4-xxx-xxx or Pxxx-xx5-xxx-xxx  (Custom Configurations)
      Pxxx-xx5-xxx-xxx or Pxxx-xxxx-6           (Standard Configurations)

      For the Win98, Win2000, WinXP with 300MHz - 1.0 GHz Processor, please use the 
      following setup file:

		DRIVERS\PRO 100 ETHERNET\82559ER\Net559ER.INF

      For WinNT with 300MHz - 1.0 GHz Processor, please use the following setup 
      file:

		DRIVERS\PRO 100 ETHERNET\82559ER\OEMSETUP.INF 

_________________________________________________________________________________________
